SECTION 27 41 16 
INTEGRATED AUDIO-VIDEO SYSTEMS AND EQUIPMENT 

GUIDE SPECIFICATION

Specifier: The Specifier/Design Professional is responsible for the accuracy of all project specifications, including system application and coordination with related sections.  This guide specification is provided as a convenience and requires editing to match actual project requirements.  CRESTRON ELECTRONICS, INC. SHALL NOT BE LIABLE FOR ANY DAMAGES ARISING OUT OF THE USE OF ANY OF ITS GUIDE SPECIFICATIONS.  For Crestron design assistance and design review please contact Sales Support Services Department at   800.237.2041 or techsales@crestron.com.

Specifer:  Please see PART 4 for a listing of products specified in this Guide Specification.

Table of Contents
1    GENERAL	3
2    PRODUCTS	3
2.1    Surface Mounted Connection Interface Type-1	3
2.1.1    Basis of Design Connection Interface	3
2.1.2    Physical	3
2.2    Surface Mounted Connection Interface Type-2	3
2.2.1    Basis of Design Connection Interface	3
2.2.2    Physical	3
3    EXECUTION	3
4    APPENDICES	3
4.1    SPECIFIED PRODUCTS	3
4.1.1    Crestron TT-100 	3
4.1.2    Crestron TT-101 	4
4.1.3    Crestron TT-110 	4
4.1.4    Crestron TT-111 	4

1	GENERAL
NOT USED in this Guide Specification. Specifier shall Specify PART 1 administrative and procedural requirements as needed.
2	PRODUCTS

2.1	Surface Mounted Connection Interface Type-1

2.1.1	Basis of Design Connection Interface

2.1.1.1	Crestron TT-100 

2.1.1.2	Crestron TT-101  

2.1.2	Physical

2.1.2.1	The Connection interface shall be available in black a finish. 

2.1.2.2	The Connection interface shall provide configurable connectivity in a flush mount tabletop unit.  

2.1.2.3	The Connection interface shall support custom combinations of cables, and an AC power outlet.   

2.2	Surface Mounted Connection Interface Type-2

2.2.1	Basis of Design Connection Interface

2.2.1.1	Crestron TT-110 

2.2.1.2	Crestron TT-111  

2.2.2	Physical

2.2.2.1	The Connection interface shall be available in black a finish. 

2.2.2.2	The Connection interface shall provide configurable connectivity in a flush mount tabletop unit.  

2.2.2.3	The Connection interface shall support custom combinations of cables.     

3	EXECUTION
NOT USED in this Guide Specification. Specifier shall Specify PART 3 On-Site work as needed.
4	APPENDICES

4.1	SPECIFIED PRODUCTS
Specifier Note: This Article includes Crestron products specified in this Guide Specification document. This Article is for reference only and should not be required in actual project manual unless included in an overall system equipment list. 
4.1.1	Crestron TT-100 

4.1.2	Crestron TT-101 

4.1.3	Crestron TT-110 

4.1.4	Crestron TT-111