SECTION 27 41 16 
INTEGRATED AUDIO-VIDEO SYSTEMS AND EQUIPMENT 

GUIDE SPECIFICATION

Specifier: The Specifier/Design Professional is responsible for the accuracy of all project specifications, including system application and coordination with related sections.  This guide specification is provided as a convenience and requires editing to match actual project requirements.  CRESTRON ELECTRONICS, INC. SHALL NOT BE LIABLE FOR ANY DAMAGES ARISING OUT OF THE USE OF ANY OF ITS GUIDE SPECIFICATIONS.  For Crestron design assistance and design review please contact Sales Support Services Department at   800.237.2041 or techsales@crestron.com.

Specifer:  Please see PART 4 for a listing of products specified in this Guide Specification.

Table of Contents
1    GENERAL	3
2    PRODUCTS	3
2.1    CONNECTION AND CONTROL INTERFACE	3
2.1.1    Basis of Design Connection Interface	3
2.1.2    Minimum Requirements	3
3    EXECUTION	3
4    APPENDICES	3
4.1    SPECIFIED PRODUCTS	3
4.1.1    Crestron FT-TS600 	3
4.1.2    Crestron FT-600 	3

1	GENERAL
NOT USED in this Guide Specification. Specifier shall Specify PART 1 administrative and procedural requirements as needed.
2	PRODUCTS

2.1	CONNECTION AND CONTROL INTERFACE

2.1.1	Basis of Design Connection Interface

2.1.1.1	Crestron FT-TS600 

2.1.1.2	Crestron FT-600
Specifier Note: The FT-600 does not include the touch screen user interface.
2.1.2	Minimum Requirements

2.1.2.1	The Connection interface shall be available in black anodized and brushed aluminum finishes. 

2.1.2.2	The Connection interface shall provide control functionality through a built-in touch screen.
Specifier Note: Touch screen requires a Crestron control processor and custom programming. FT-600 does not include the touch screen user interface.
2.1.2.2.1	Touch Screen UI shall be powered via a PoE connection. 

2.1.2.2.2	Touch screen UI shall communicate with control processor via PoE connection.  

2.1.2.3	The Connection interface shall provide configurable connectivity in a flush mount tabletop unit.  

2.1.2.4	The Connection interface shall utilize a universal cutout size that will fit other interfaces from same manufacturer.  

2.1.2.5	The Connection interface shall support custom combinations of pullout cables, cable retractors, connector panels, and AC power outlets.      

3	EXECUTION
NOT USED in this Guide Specification. Specifier shall Specify PART 3 On-Site work as needed.
4	APPENDICES

4.1	SPECIFIED PRODUCTS

4.1.1	Crestron FT-TS600 

4.1.2	Crestron FT-600